Dongguan Hai Mi Electronic Technology Limited.

DC Brushless Water Pump
	

	· Product Parameter

	Model
Character
	HM2502-1

	
Working voltage range
	5VDC-12VDC

	Optional rated power
	0.5~3W

	Optional static water head
	0.5~2.5 meters

	
Optional static flow rate
	0.5 ~ 2.5L/min

	
Lifespan
	Continuous operation under normal working surrounding＞20000H

	
Working Environment
	PH value: PH5-10(weak acid and weak base), workable in water and on land.

	
Max noise
	Under normal working condition,(1meter over the test instrument)＜35dB

	Other optional special functions
	Water shortage protection, over-voltage protection, over-current protection, blocking protection, 0-5V speed control, PWM speed control, FG signal feedback, etc.

	
Max working temperature
	Under room temperature surroundings, fluid medium temperature≤100℃

	

Application
	(Automatic) Coffee machine, automatic teapot, juice extractor, beverage machine, wine set, water dispenser, humidifier, pet drinking water dispenser, small fountain, aquarium, solar water circulation system, soil-less cultivation, foot bath basin, crafts, etc. 

	
Color
	 Black (Can be customized according to customer`s requirement)

	

Outlet direction
	Can be adjustable at any angle

	
Dimension
	IP grade
	Inlet
	Outlet
	Remarks

	Length（mm）
	Width（mm）
	Height（mm）
	
	OD（mm）
	ID（mm）
	OD（mm）
	ID（mm）
	Inlet and outlet have anti-slip strip

	
41.5

	26.2
	37.0
	IP67
	10.0
	7.0
	7.0
	4.0
	

	· Outside View
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	· Curve Graph
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Remarks: The graph is just for your reference, the final one comes with the customer required specifications.

	· Photo for you reference
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https://haimidcpump.en.alibaba.com
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