Dongguan Hai Mi Electronic Technology Limited.

DC Brushless Water Pump
	

	· Product Parameter

	Model
Character
	HM3001-2

	
Working voltage range
	5VDC-24VDC

	Optional rated power
	0.3~4W

	Optional static water head
	0.5~2 meters

	
Optional static flow rate
	1~3.5L/min

	
Lifespan
	Continuous operation under normal working surrounding＞20000H

	
Working Environment
	PH value: PH5-10(weak acid and weak base),workable in water, submersible pump

	
Max noise
	Under normal working condition,(1meter over the test instrument)＜35dB

	Other optional special functions
	Water shortage protection, over-voltage protection, over-current protection, blocking protection, 0-5V speed control, PWM speed control, FG signal feedback, UV LED disinfection lamp, etc.

	
Max working temperature
	Under room temperature surroundings, fluid medium temperature≤70℃

	
Application
	Water dispenser, humidifier, pet drinking water dispenser, small fountain, aquarium, solar water circulation system, soilless cultivation, hydropnics, decorative potted plants, foot bath basin, small medical equipment, crafts, etc. 

	
Color
	 White/ Black (Can be customized according to customer`s requirement)

	
Outlet direction
	Can be adjustable at any angle

	
Dimension
	IP grade
	Inlet
	Outlet
	Remarks

	Length（mm）
	Width（mm）
	Height（mm）
	
	OD（mm）
	ID（mm）
	OD（mm）
	ID（mm）
	Outlet have anti-slip strip

	
41.6

	37.0
	44.5
	IP68
	-------
	-------
	8.5
	5.5
	

	· Outside View
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	· Curve Graph
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Remarks: The graph is just for your reference, the final one comes with the customer required specifications.

	· Photo for you reference
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Two colors for choosing




https://haimidcpump.en.alibaba.com
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