Dongguan Hai Mi Electronic Technology Limited.

DC Brushless Water Pump
	

	· Product Parameter

	Model
Character
	HM3207-1

	
Rated working voltage
	12VDC

	working voltage range
	 10VDC-14VDC

	Rated power
	     4.8W 

	
Static water head
	3 meters

	
Static flow rate
	240 L/H

	
Lifespan
	Continuous operation under normal working surrounding＞20000H

	
Working Environment
	PH value: PH5-10(weak acid and weak base), workable both on land and in water.

	
Max noise
	Under normal working condition,(1meter over the test instrument)＜35dB

	
Max working temperature
	Under room temperature surroundings, fluid medium temperature≤70℃

	


Application
	Water circulation of humidifier, air conditioner and fans, hydroponics, smart garden herbs, garden fountain, aquarium, water tank, fish pond, solar water circulation, water circulation of home appliance, etc.

	
Color
	Black (Can be customized according to customer`s requirement)

	

Outlet direction
	Can be adjustable at any angle

	

Dimension
	IP grade
	Inlet
	Outlet
	Remarks

	
Length
（mm）
	
Width（mm）
	
Height（mm）
	
	OD（mm）
	ID（mm）
	OD（mm）
	ID（mm）
	Inlet and outlet have anti slip strip

	
54.4

	52.0
	40.8
	IP68
	8.5
	6.0
	8.5
	6.0
	

	· Outside View

	

	· Curve Graph

	
Remarks: The graph is just for your reference, the final one comes with the customer required specifications.  

	· Photo for your reference

	                  









 https:hmdcpump.en.alibaba.com
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