Dongguan Hai Mi Electronic Technology Limited.

DC Brushless Water Pump
	

	· Product Parameter

	Model
Character
	             HM4510-1 ( Three phase pump)

	
Working voltage range
	6VDC-24VDC

	Rated power
	   20~60 W 

	
Static water head range
	1~6 meters 

	
Static flow rate range
	20~ 50 L/min 

	
Lifespan
	Continuous operation under normal working surrounding＞20000H

	
Working Environment
	PH value: PH5-10(weak acid and weak base), workable both on land and in water.

	
Max noise
	Under normal working condition,(1meter over the test instrument)＜40dB

	
Other optional special functions

	Water shortage protection, over-voltage protection, over-current protection, blocking protection, 0-5V speed control, PWM speed control, FG signal feedback, etc.

	
Max working temperature
	Under room temperature surroundings, fluid medium temperature≤100℃

	        Application
	
Water circulation oxygenation, swimming pool spa heating system, medical equipment, beauty equipment, mobile bath machine, (solar ) fountain,  aquarium, water tank, fish pond, solar water circulation, water circulation of home appliance, crafts, etc.


	
Color
	[bookmark: _GoBack]Black (Can be customized according to customer`s requirement)

	
Outlet direction
	Can be adjustable at any angle

	

Dimension
	IP grade
	Inlet
	Outlet
	Remarks

	
Length
（mm）
	
Width（mm）
	
Height（mm）
	
	OD（mm）
	ID（mm）
	OD（mm）
	ID（mm）
	It has three output 

	
96.5

	86.0
	--
	IP68
	25.2
	18.3
	--
	10.0
	

	· Outside View

	[image: 6573cf17-1725-4649-a76c-717cc3711cb7]

	· [image: ]Curve Graph

	








  

Remarks: The graph is just for your reference, the final one comes with the customer required specifications.  

	· Photo for your reference

	[image: 63f94859-a104-4724-bc62-06747e0a9322] 




https://haimidcpump.en.alibaba.com
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