Dongguan Hai Mi Electronic Technology Limited.

DC Brushless Water Pump
	

	· Product Parameter

	Model
Character
	                HM651205-5 ( Three phase pump)

	
Working voltage range
	9VDC-13.5VDC

	Rated voltage
	12VDC

	Rated power
	≤5W 

	
Max static water head
	1.6±10% Meters

	
Static flow rate
	＞550mL/min@1.2m

	
Lifespan
	Continuous operation under normal working surrounding＞20000H

	
Working Environment
	PH value: PH5-10(weak acid and weak base), workable both in water and on land. 

	
Max noise
	Under normal working condition,(1meter over the test instrument)＜30dB

	Max working temperature
	Under room temperature surroundings, fluid medium temperature≤70℃

	
Other optional special functions

	Water shortage protection, over-voltage protection, over-current protection, blocking protection, 0-5V speed control, PWM speed control, FG signal feedback, etc.

	Application
	Air conditioner drainage system, portable air conditioner drainage system, small electrical appliance drainage system, potted plant decoration, hydroponics, humidifier, small fountain, aquarium, small medical equipment, handicrafts, etc. 

	
Color
	Black (Can be customized according to customer’s requirement)

	
Outlet direction
	Can be adjustable at any angle

	
Dimension
	IP grade
	Inlet
	Outlet
	Remarks

	
Length
（mm）
	
Width（mm）
	
Height（mm）
	
	OD（mm）
	ID（mm）
	OD（mm）
	ID（mm）
	Outlet has anti-slip strip.

	
94.3

	74.0
	70.0
	IP67
	20.0
	10.5
	14.0
	9.0
	

	· Outside View

	 










	· Curve Graph

	      







      




Remarks: The graph is just for your reference, the final one comes with the customer required specifications.  

	· Photo for your reference

	           




 https://haimidcpump.en.alibaba.com
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