Dongguan Hai Mi Electronic Technology Limited.

DC Brushless Water Pump
	

	· Product Parameter

	Model
Character
	HM2501-1

	
Working voltage range
	5VDC-12VDC

	Optional rated power
	0.5~3W

	Optional static water head
	0.5~2.5 meters

	
Optional static flow rate
	0.5 ~ 2.5L/min

	
Lifespan
	Continuous operation under normal working surrounding＞20000H

	
Working Environment
	PH value: PH5-10(weak acid and weak base), workable on land. NON submersible.

	
Max noise
	Under normal working condition,(1meter over the test instrument)＜35dB

	Other optional special functions
	Water shortage protection, over-voltage protection, over-current protection, blocking protection, 0-5V speed control, PWM speed control, FG signal feedback, etc.

	
Max working temperature
	Under room temperature surroundings, fluid medium temperature≤100℃

	

Application
	[bookmark: _GoBack](Automatic) Coffee machine, automatic teapot, juice extractor, beverage machine, wine set, water dispenser, humidifier, pet drinking water dispenser, small fountain, aquarium, solar water circulation system, crafts, etc. 

	
Color
	 White (Can be customized according to customer`s requirement)

	

Outlet direction
	Can be adjustable at any angle

	
Dimension
	IP grade
	Inlet
	Outlet
	Remarks

	Length（mm）
	Width（mm）
	Height（mm）
	
	OD（mm）
	ID（mm）
	OD（mm）
	ID（mm）
	Inlet and outlet have anti-slip strip

	
41.5

	26.2
	37.0
	IP67
	10.0
	7.0
	7.0
	4.0
	

	· Outside View

	[image: ]       


	· Curve Graph

	[image: ]         










Remarks: The graph is just for your reference, the final one comes with the customer required specifications.

	· Photo for you reference

	                         [image: ]




https://haimidcpump.en.alibaba.com
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