Dongguan Hai Mi Electronic Technology Limited.

DC Brushless Water Pump
	

	· Product Parameter

	Model
Character
	                HM90120W-1( Three phase pump)

	
Working voltage range
	10VDC-26VDC

	Optional rated voltage
	                    6VDC/12VDC/24VDC (Other rated voltage can be supplied)

	Rated power
	40~120 W 

	
Static water head
	1~6 meters

	
Static flow rate
	10~ 60 L/min

	
Lifespan
	Continuous operation under normal working surrounding＞20000H

	
Working Environment
	PH value: PH5-10(weak acid and weak base), workable in water, submersible pump.

	
Max noise
	Under normal working condition,(1meter over the test instrument)＜45dB

	Max working temperature
	Under room temperature surroundings, fluid medium temperature≤70℃

	
Other optional special functions

	Water shortage protection, over-voltage protection, over-current protection, blocking protection, 0-5V speed control, PWM speed control, FG signal feedback, etc.

	Application
	Sewage systems, portable handheld water stick, solar-powered hot water circulation systems, solar pool heating systems, household appliance water circulation systems, fountains, aquariums, crafts, etc.

	
Color
	Black (Can be customized according to customer’s requirement)

	
Outlet direction
	Can be adjustable at any angle

	
Dimension
	IP grade
	Inlet
	Outlet
	Remarks

	
Length
（mm）
	
Width（mm）
	
Height（mm）
	
	OD（mm）
	ID（mm）
	OD（mm）
	ID（mm）
	Outlet has threads.

	
140.0

	120.0
	--
	IP68
	120
	--
	50
	G1″ threads
	

	· Outside View

	

	· Curve Graph

	
Remarks: The graph is just for your reference, the final one comes with the customer required specifications.  

	· Photo for your reference
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