Dongguan Hai Mi Electronic Technology Limited.

DC Brushless Water Pump
	

	· Product Parameter

	Model
Character
	                HM5012-1( Three phase pump)

	
Working voltage range
	12VDC-24VDC

	Rated power
	15~90 W

	
Static water head
	2~14 meters

	
Static flow rate
	10~ 30 L/min

	
Lifespan
	Continuous operation under normal working surrounding＞20000H

	
Working Environment
	PH value: PH5-10(weak acid and weak base), workable on land only. 

	
Max noise
	Under normal working condition,(1meter over the test instrument)＜45dB

	Max working temperature
	Under room temperature surroundings, fluid medium temperature≤75℃ 

	
Other optional special functions

	Water shortage protection, over-voltage protection, over-current protection, blocking protection, 0-5V speed control, PWM speed control, FG signal feedback, etc.

	Application
	Sewage discharge,oil-water separator, solar pool heating system, solar spa heating system, solar water heater, hot water circulation, Electric Vehicle Engine, water coolant of vehicle, car washing, irrigation, milling machine, drilling machine, turning lathe, fountain, aquarium, water tank, fish pond, solar water circulation, water circulation of home appliance, crafts, etc.

	
Color
	Black (Can be customized according to customer’s requirement)

	
Outlet direction
	Can be adjustable at any angle

	
Dimension
	IP grade
	Inlet
	Outlet
	Remarks

	
Length
（mm）
	
Width（mm）
	
Height（mm）
	
	OD（mm）
	ID（mm）
	OD（mm）
	ID（mm）
	Inlet and outlet have screw threads.

	
79.0

	57.0
	129.0
	IP67
	G1/2″ threads
	15.0
	G1/2″ threads
	15.0
	

	· Outside View

	

	· Curve Graph
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Remarks: The graph is just for your reference, the final one comes with the customer required specifications.  

	· Photo for your reference
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