Dongguan Hai Mi Electronic Technology Limited.

DC Brushless Water Pump
	

	· Product Parameter

	Model
Character
	                HM6003-1( Three phase pump)

	
Working voltage range
	12VDC-48VDC

	Rated power
	12~80 W 

	
Static water head
	2~20 meters

	
Static flow rate
	10~ 28 L/min

	
Lifespan
	Continuous operation under normal working surrounding＞20000H

	
Working Environment
	PH value: PH5-10(weak acid and weak base), workable on land only. 

	
Max noise
	Under normal working condition,(1meter over the test instrument)＜45dB

	Max working temperature
	Under room temperature surroundings, fluid medium temperature≤80℃

	
Other optional special functions

	Water shortage protection, over-voltage protection, over-current protection, blocking protection, 0-5V speed control, PWM speed control, FG signal feedback, etc.

	Application
	Solar water circulation systems, solar water heating systems, solar pool heating systems, water heater pressure boosters, high-rise building water pressure boosters, sewage systems, lathe washing systems, (EV)Water circulation cooling systems, car wash systems, household appliance water circulation systems, agriculture irrigation, fountain, aquarium, water tank, fish pond, crafts, etc.

	
Color
	Black (Can be customized according to customer’s requirement)

	
Outlet direction
	Can be adjustable at any angle

	
Dimension
	IP grade
	Inlet
	Outlet
	Remarks

	
Length
（mm）
	
Width（mm）
	
Height（mm）
	
	OD（mm）
	ID（mm）
	OD（mm）
	ID（mm）
	Inlet and outlet have anti-slip strips.

	
96.5

	71.0
	85.5
	IP68
	30.0
	20.0
	20.0
	12.3
	

	· Outside View

	      

	· Curve Graph

	      











Remarks: The graph is just for your reference, the final one comes with the customer required specifications.  

	· Photo for your reference

	        
     




 https://haimidcpump.en.alibaba.com
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