Dongguan Hai Mi Electronic Technology Limited.

DC Brushless Water Pump
	

	· Product Parameter

	Model
Character
	HM3811-1（Three-phase pump）

	
Working voltage range
	5VDC-24VDC

	Optional rated power
	3-30 W

	Optional static water head
	0.5~11 meters

	
Optional static flow rate
	5-10 L/min

	
Lifespan
	Continuous operation under normal working surrounding＞20000H

	
Working Environment
	PH value: PH5-10(weak acid and weak base),workable in water, submersible pump

	
Max noise
	Under normal working condition,(1meter over the test instrument)＜35dB

	Other optional special functions
	Water shortage protection, over-voltage protection, over-current protection, blocking protection, 0-5V speed control, PWM speed control, FG signal feedback, etc.

	
Max working temperature
	Under room temperature surroundings, fluid medium temperature≤70℃

	
Application
	Head therapy instrument, mobile bath machine, mobile air conditioner, small fountain, aquarium, solar water circulation system, soil-less cultivation, car refrigerator, car washing, hydroponics, decorative potted plants, foot bath basin, small medical equipment, fountain, aquarium, home appliance, crafts, etc. 

	
Color
	 White/ Black (Can be customized according to customer`s requirement)

	
Outlet direction
	Can be adjustable at any angle

	
Dimension
	IP grade
	Inlet
	Outlet
	Remarks

	Length（mm）
	Width（mm）
	Height（mm）
	
	OD（mm）
	ID（mm）
	OD（mm）
	ID（mm）
	Inlet has filter hood.

	
109.0

	50.0
	57.0
	IP68
	33.0
	-------
	11.0
	6.0
	

	· Outside View
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	· Curve Graph
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Remarks: The graph is just for your reference, the final one comes with the customer required specifications.

	· Photo for you reference
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https://haimidcpump.en.alibaba.com
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